GARMIN iQue Software Upgrade Information
Software Version 5.2.1.r6 EFIGS

http://www.garmin.com

------------------------------------------------------------

WARNINGS:
    If this software is uploaded to a GPS unit other than the product for
    which it is designed, you will not be able to operate that unit.

------------------------------------------------------------

Instructions for uploading the new software to your iQue 3600 using Microsoft
Windows 98/ME/2000/XP:

1.  Ensure that the current software is Release 3 or later. The Release 6 EFIGS update
    works only when Release 3 software or later is resident in the unit.

    A. Go to the Launcher (tap on the house icon in the lower left corner).
    B. Tap the menu icon (it is the 'down-arrow' icon just to the right of the house
       icon in the lower left corner).
    C. A drop down menu will appear.
    D. Tap the Info... menu item.
    E. Tap the Version button at the bottom of the screen and check that the second
       line of the screen is v.5.2.1r3 or later.

2.  Download and save the iQue3600withEFIGS_Release6.zip update file to a location
    on your computer.  This file will need to be located later so please locate 
    this in a readily accessible folder.

3.  Place the iQue in the cradle and perform a HotSync on the unit to backup 
    any of your current data.  Please ensure that the iQue is fully charged 
    before proceeding with the software update process.

4.  Perform a Hard Reset of the unit.  To perform this procedure you will need 
    the reset tip tool, which may be unscrewed from the head of the Stylus that 
    came with your iQue.  The following instructions are also included on page 
    1.6 of the iQue 3600 Integrated Handheld Operating Instructions manual.

    A. With the unit turned off, press and hold in the reset button on the back
       of the unit using the reset tip tool.
    B. Continue to hold in the reset button while you press and hold the power 
       button.
    C. While holding in the power button, remove the reset tool from the reset 
       hole.  
    D. Continue holding the power button until the Palm logo appears on the 
       screen.  
    E. Once the Palm logo appears, release the power button.
    F. Press the up button when prompted to confirm the erase of user data. 

5.  A new user will need to be created for use during the software update process.  

    A. Start by launching the Palm Desktop application
    B. Go to the Tools menu, then select Users... to display a list of the 
       current users.
    C. Click on the New... button to display the New User window.
    D. Enter a unique name for the user, such as Release6EFIGS, then click OK.
    E. Close out of the Users window by clicking OK.

6.  If you are using Intellisync Lite or another synchronization program, from 
    within that program configure your new user to synchronize with the Palm 
    Desktop or any available alternative that does not contain your primary data.  

7.  Install the software update to the new user (Release6EFIGS).

    A. Double click the iQue3600withEFIGS_Release6.zip, then unzip to a 
       location that can be easily found, such as the Desktop.  There will be 
       three files: Updater.prc, UpdaterData.pdb, and a copy of these 
       instructions (iQue 3600 EFIGS Release 6.txt).
    B. Double click the Updater.prc file.  This will open the Palm Desktop 
       Install Tool.  
    C. Select the new user that you have created (Release6EFIGS), and click OK. 
    D. Double click the UpdaterData.pdb file to place it in the Palm Desktop 
       Install Tool. 
    E. Close the Palm Desktop Install Tool by clicking Done, then click OK.

8.  Place the iQue in the cradle and initiate a HotSync.  A Select User window 
    will appear.  Select the new user (Release6EFIGS) that you have created for 
    the update.  The Updater.prc and UpdaterData.pdb files will then be 
    installed on the iQue.

9.  You may update the iQue while it is in or out of the cradle. However, once
    the update has begun, do not place the iQue into or remove the iQue from the
    cradle. This could interrupt the update and require you to send your unit to
    Garmin for repair.  Also, it is very important that the iQue does not lose
    power during the update process, so please verify that the battery is fully
    charged if you won't be powering it externally. Failure to charge the iQue
    fully prior to updating the software may result in a permanent loss of the
    OS requiring you to send your unit to Garmin for repair.

10. Locate the application called Updater.  It can be found under the category 
    of All.  Once you have located the Updater application, tap on it once.  
    Then follow the on-screen instructions.  

11. After about 4 minutes, the unit will reset itself.  Follow the on-screen
    setup instructions.

12. Verify that the software update was successful.

    A. Go to the Launcher (tap on the house icon in the lower left corner) 
    B. Tap the menu icon (it is the "down-arrow" icon just to the right of the
       house icon in the lower left corner).  
    C. A drop down menu will appear.
    D. Tap the Info... menu item.
    E. Tap the Version button at the bottom of the screen.  The update was 
       successful if the second line of the screen displays Palm OS software 
       v.5.2.1r6.

13. If you are using Intellisync Lite or another synchronization program, from 
    within that program make sure the current user is set to the User name that 
    you have been previously using to identify your iQue.

14. To restore your previous information to the iQue, place the iQue in the 
    cradle, then perform a HotSync. A window will appear asking to select a 
    User.  Select the User name that you have been previously using to 
    identify your iQue on your PC, and your information will be restored to 
    the iQue.

15. Delete the temporary user (Release6EFIGS) by going back to the Users window in 
    the Palm Desktop.  Select the user, click Delete... then click YES to 
    delete it.

------------------------------------------------------------

Changes Made from Versions 5.2.1.r5 to 5.2.1.r6:

Que Applications

1. Corrected a problem that caused lockups in QueTurns on certain routes.
2. Improved 'Find Along Route' in QueFind for metric values.

------------------------------------------------------------

Changes Made from Versions 5.2.1.r4 to 5.2.1.r5:

Routing:
1.  Improved routing support for tolled roads particularly in Austria and Switzerland.


------------------------------------------------------------

Changes Made from Versions 5.2.1.r3 to 5.2.1.r4:

GPS:
1.  Added support for QueAPILib 3.0.

Mapping:
1.  Improved the display of waypoints by re-highlighting them after zooming,
    if they were previously highlighted.
2.  Changed the active track log color to improve visibility.
3.  Corrected the display and highlighting of waypoints after creating them
    from QueMap.
4.  Corrected the Indonesian Southern grid, which had been using the wrong
    longitude of origin.

Que Applications:
1.  Added support for 24-hour time display, as well as other PalmOS supported
    formats, in certain Que applications.
2.  Improved the display of pre-1990 dates in certain Que applications.
3.  Increased the maximum waypoint limit from 4096 to approximately 10000.
4.  Corrected a problem with the map’s zoom popup that could sometimes occur in
    the Address Book application.
5.  Corrected handling of next appointment field in QueClock when private records
    are used.
6.  Corrected a problem that caused certain applications to exit if the escape
    button was pressed while a Turn Popup window was being displayed.  Now it just
    closes the Turn Popup.
7.  Corrected a problem where the unit wouldn’t auto-off if an alarm occurred while
    in QueVoice and the alarm message wasn’t manually dismissed.
 
PIM:
1.  Corrected a problem with the manual creation of waypoints in the Address Book
    while using the Indonesian Irian, Indonesian Southern, Swiss, Taiwan, Dutch,
    and Qatar (QNG) grids.
2.  Updated the First Aid waypoint symbol.

SD/MMC:
1.  Improved handling of large memory cards in CardInfo.

Searching:
1.  Corrected a problem searching Fishing HotSpots maps.

System:
1.  Corrected a problem with the Voice Guidance volume not always staying at
    the value at which it was set.
2.  Updated some of the EFIGS text translations.
3.  Broadcast the sysExternalConnectorAttachEvent & sysExternalConnectorDetachEvent
    PalmOS notifications when something is attached to or detached from the
    Universal Connector.

----------

Changes Made from Version Release 3 English-only to Release 3 EFIGS

- Added support for French, Italian, German, and Spanish languages.