GARMIN iQue 3600a Software Upgrade Information
Software Version 5.2.1.r3

http://www.garmin.com

------------------------------------------------------------

WARNINGS:
    If this software is uploaded to a GPS unit other than the product for
    which it is designed, you will not be able to operate that unit.

------------------------------------------------------------

Instructions for uploading the new software to your iQue 3600a using Microsoft
Windows 98/ME/2000/XP:

1. Download and save the iQue3600a_Release3.zip update file to a location on 
   your computer. This file will need to be located later, so please locate this 
   in a readily accessible folder.

2. Place the iQue in the cradle and perform a HotSync on the unit to back up 
   any of your current data. Please ensure that the iQue is fully charged before 
   proceeding with the software update process.

3. Perform a Hard Reset of the unit. To perform this procedure, you will need 
   the reset tip tool, which may be unscrewed from the head of the stylus that 
   came with your iQue. The following instructions are also included on page 1.6 
   of the iQue 3600a Integrated Handheld Operating Instructions manual.

   A. With the unit turned off, press and hold in the reset button on the back 
      of the unit using the reset tip tool.
   B. Continue to hold in the reset button while you press and hold the power 
      button.
   C. While holding in the power button, remove the reset tool from the reset 
      hole.
   D. Continue holding the power button until the Palm logo appears on the 
      screen.
   E. Once the Palm logo appears, release the power button.
   F. Press the up button when prompted to confirm the erase of user data.

4. A new user for the software update will need to be created for use during 
   the software update process.

   A. Start by launching the Palm Desktop application.
   B. Go to the Tools menu, then select Users... to display a list of the 
      current users.
   C. Click on the New... button to display the New User window.
   D. Enter a unique name for the User, such as Release3, and then click OK.
   E. Close out of the Users window by clicking OK. 

5. Install the software update to the new user (Release3).

   A. Double click the iQue3600a_Release3.zip, then unzip to a location that 
      can be easily found, such as the Desktop. There will be three files: 
      Updater.prc, UpdaterData.pdb, and a copy of these instructions (iQue 3600a 
      Release 3.txt).
   B. Double click the Updater.prc file. This will open the Palm Desktop Install 
      Tool.
   C. Select the new user that you have created (Release3), and click OK.
   D. Double click the UpdaterData.pdb file to place it in the Palm Desktop 
      Install Tool.
   E. Close the Palm Desktop Install Tool by clicking Done, then click OK.

6. Place the iQue in the cradle and initiate a HotSync. A Select User window 
   will appear. Select the new user (Release3) that you have created for the 
   update. The Updater.prc and UpdaterData.pdb files will then be installed on 
   the iQue.

7. Remove the iQue from the cradle. It is very important that the iQue's 
   battery does not run out during the updating process, so please verify that 
   it is fully charged. Failure to charge the iQue fully prior to updating the 
   software may result in a permanent loss of the OS requiring you to send your 
   unit to Garmin for repair.

8. Locate the Application called Updater. It can be found under the category of 
   All. Once you have located the Updater Application, tap on it once. Then 
   follow the on-screen instructions.

9. After 5 to 7 minutes, the unit will reset itself. Follow the on-screen 
   setup instructions.

10. Verify that the software update was successful.

    A. Go to the Launcher (tap on the house icon in the lower-left corner).
    B. Tap the menu icon (it is the icon just to the right of the house icon in 
       the lower-left corner).
    C. A drop-down menu will appear.
    D. Tap the Info... menu item.
    E. Tap the Version button at the bottom of the screen. The update was 
       successful if the second line of the screen displays Palm OS software 
       v.5.2.1r3.

11. To restore your previous information to the iQue, place the iQue in the 
    cradle, then perform a HotSync. A window will appear asking to select a 
    User. Select the User name that you have been previously been using to 
    identify your iQue on your PC, and your information will be restored to 
    the iQue.

12. Delete the temporary user (Release3) by going back to the Users window in 
    the Palm Desktop. Select the user, click Delete... then click YES to delete 
    it.


------------------------------------------------------------

Changes Made from Versions 5.2.1.r2 to 5.2.1.r3:

Navigation/Routes/Routing:
1. Fixed issue with the "Find Along Route" option.

Aviation:
1. Fixed issue when viewing airspace frequencies for a danger area

------------------------------------------------------------

Changes Made from Versions 5.2.1.r1 to 5.2.1.r2:

Audio: 
1. Improved voice guidance playback to remove stuttering.

Aviation:
1. Improved suppression of nuisance terrain and obstacle alerts.
2. Improved the handling of multiple simultaneous airspace alerts.
3. Improved Aviation Map Review Page display when opened from the runway tab.
4. Improved the display of airspace text on the Aviation Nearest Airspace list 
   and details pages.
5. Updated the ETE calculations so the values match the Garmin panel-mount 
   products’ ETE values.
6. Corrected the Terrain Preference Page so the Terrain Alert settings now get 
   saved.
7. Corrected the Aviation Review Page handling of the details for runway 
   waypoints for airport approaches.
8. Corrected some QueE6B calculations.
9. Corrected some minor problems with the Aviation Points page.
10. Corrected a problem that causes some incorrect leg data after removing a 
    waypoint from a route while a Goto is active.
11. Corrected a problem where runway extensions would draw at the incorrect 
    airport on a multi-airport route if the map was fully decluttered.
12. Corrected a problem that could corrupt the active route waypoint after 
    passing the FAF waypoint and sequencing onto the MAP-to-FAF approach leg. 
    This could cause invalid distance, bearing, and time data to display.
13. Corrected a problem that could sometimes cause airports to get listed 
    twice in the Aviation Nearest Weather list.

GPS: 
1. Added support for QueAPILib 2.0.

Navigation/Routes/Routing:
1. Added support for closing the Turn Popup Page using the Enter and 
   Escape keys.
2. Added support for routing to recently found points even if detailed map 
   data has been removed.
3. Added support to the Active Route Page for routes with more than 21 points.

Mapping: 
1. Improved the text size for the 'Wpt Next' and 'Wpt Dest' map overlay 
   fields.
2. Corrected a problem switching from Track Up orientation to North Up when 
   the map was zoomed to a level above the "Track Up Below..." setting.

Que Applications: 
1. Added support for 24-hour time display, as well as other PalmOS supported 
   formats, in certain Que applications.
2. Improved the display of pre-1990 dates in certain Que applications.
3. Corrected a problem with the map’s zoom popup that could sometimes occur in 
   the Address Book application.

SD/MMC: 
1. Improved handling of large memory cards in CardInfo.

System: 
1. Improved battery management.
